Diagram

Description automatically generated**Column Placements (red Xs) *for all floors.*:**

* Place columns inside walls at A2, A4 on the left.
* Place columns inside walls at D2 and D4 on the right.
* Place columns at positions 2 and 4 offset from the right by 6.45 meters. These columns also will reside inside walls as shown.

**Adjustments:**

**Floor 2**

**Diagram

Description automatically generated**

The second bedroom had been reduced in size in the plans you sent us. Please adjust the wall marked in blue to 3.88 m. The gray outlined wall, circled in red is the corrected location after the expansion.

**Adjustments**

Diagram, engineering drawing

Description automatically generated**Floors 3-4: part 1**

The terrace for the living room has been reduced to 3.66m in length as shown above. The gray outlined walls show the new dimensions after reduction. Please install a door at the location shown in red.

**Adjustments**

Diagram

Description automatically generated**Floors 3-4: part 2**

Expand the master bathroom on the 3-4 floor plan by 1 meter by reducing 1 meter from bedroom 3 in the marked location. The gray outline shows the new dimensions. The new wall after expansion is colored in blue.

**Multipurpose floor adjustments**

Please see the next page for the adjustments to the multipurpose floor.